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	1.
	Identification of the mixture and of the company/undertaking



[bookmark: _Hlk62559550]1.1 Product identifier:  Hexol Synline SprintPlus Maxx 0W30 API SN/CF 
1.2 Relevant identified uses of the mixture and uses advised against 
      Relevant identified uses: engine oil. 
      Restrictions on use: any other uses not recommended are forbidden. 
1.3 Details of the supplier of the safety data sheet: 
      S.C. HEXOL LUBE S.R.L.
      Adress: Paleu commune, Ardealului street, no. 1A, Bihor county
      Phone/Fax: +4 0259 449 203/+4 0259 428 299
      E-mail: office@hexol.com
1.4 Emergency telephone number 
      Phone: +4 0259 454 216; +4 0259 449 203; 8-16h on workdays.

	2. Hazards’ identification

	2.1 Classification of the mixture

	      Classification of the mixture according to Regulation 1272/2008/EC

	      Not required.


2.2 Label elements: Labelling according to Regulation 1272/2008/EC
      Product identification: Trade name:Hexol Synline SprintPlus Maxx 0W30 API SN/CF
	      Precautionary statements:
      P 273: Avoid release in the environment.
      P 501: Dispose of contents/container in accordance with national/international regulation.
2.3 Other hazards: 
      Hazard description: If usual precautions are taken when handling products containing mineral   
      oils, the instructions for handling (Chapter 7) and personal protection (Chapter 8) are respected, 
      there are no known hazards.


	3. Composition/information on ingredients
3.2 Mixtures
      Chemical description: Mixture of refined mineral base oils containing additives.

	     
	Name
	EINECS No.
	CAS No.
	REACH No.
	Classification according to the Regulation (CE) Nr. 1272/2008 [CLP]
	Conc.%

	Mineral Oil
	276-738-4
	72623-87-1
	-
	-

	90-95

	Benzenesulfonic acid, mono-C16-24- alkyl derivs., calcium salts 
	274-263-7
	70024-69-0
	01-2119492616-28-xxxx
	H317
	0.85-1.27

	Phosphorodithioic acid, mixed O,O-bis(2-ethylhexyl and iso-Bu and iso-Pr) esters, zinc salts
	288-917-4
	85940-28-9
	01-2119521201-61-xxxx
	H315, H318, H411
	0.85-1.27

	Benzenamine, N-phenyl-, reaction products with 2,4,4-trimethylpentene 
	270-128-1
	68411-46-1
	01-2119491299-23-xxxx
	H361
	0.42-0.85

	Reaction product of cocoalkyldiethanolamides and oalkylmonoglycerides and molybdenumtrioxide 
	430-380-7
	445409-27-8
	01-0000017666-61-XXXX 

	H411
	˂0.08


 
	
	
	
	
	
	

	      For full text of each relevant P-, H- phrase and Hazard classes and cat. see Section 16.

	

	4. First aid measures

	4.1 Description of first aid measures
      General advice: Remove victim from exposure site. Ensure that the person has fresh air. Lay 
      person in lateral, stable position and keep warm. In case of irregular breathing or respiratory arrest 
      apply artificial respiration.
      First aid responders must avoid exposure. Proper respiratory protection will be used. In case of
      respiratory arrest mechanical ventilation should be provided. Do not use mouth to mouth 
      resuscitation. Remove all contaminated clothing immediately.
      Inhalation: In case of accident by inhalation, transport the victim out of the contaminated area and 
      leave to rest. If symptoms persist, seek medical advice.
      Skin contact: Remove contaminated clothing and wash the skin thoroughly with soap and water. If  
      symptoms persist, seek medical advice.
      Eye contact: Wash thoroughly with water for at least 10 minutes. If symptoms persist, seek medical  
      advice.
      After ingestion: An unconscious person should never be forced to swallow. Vomiting will not be
      induced. Seek medical advice immediately.

	4.2 Most important symptoms and effects, both acute and delayed - No data available.
4.3 Indication of any immediate medical attention and special treatment needed – Treat  
      symptomatically

	
	
	
	
	

	

	5. Fire-fighting measures
5.1 Fire extinguishing equipment
      Suitable fire-extinguishing equipment: Use foam, carbon dioxide, dry powder, water and sand 
      dispersants. 
      Unsuitable extinguishing media: Never use a powerful water jet.
5.2 Special hazards arising from the mixture 
      Hazardous combustion products: in case of fires carbon dioxide, carbon monoxide, sulphur  
      oxides, phosphor oxides, various hydrocarbons and soot can be formed. 
5.3 Recommendations for firefighters 
      In case of fires self-contained breathing apparatus will be used. Special protective equipment:  
      According to the existing firefighting regulations.
      Further information: 
      Collect contaminated firefighting water separately. It must not enter the sewer system.     
      Combustion residues and the contaminated water use in extinguishing the fire must be disposed of 
      in accordance with local regulations.

6. Accidental release measures	
6.1 Personal precautions, protective equipment and emergency procedures
      Use personal protective equipment. Keep away people without protective equipment or untrained  
      people. Avoid contact with skin and eyes. Avoid breathing vapours or spray mist. Wear respiratory 
      protective equipment.
      Personal precautions: see Section 8.
6.2 Environmental precautions:	
      Confine spills to prevent material from entering sewers, watercourses, drains and into soil. In case 
      of environmental release notify relevant authority.
6.3 Methods and material for fire containment and cleaning up
      On soil: Eliminate all ignition sources. Collect spillage. Contain the rest or small quantities using 
      absorbent materials: sand, earth or other suitable absorbents. Dispose of materials and solid residues  
      according to local regulations. 
      In water: Confine the spillage.  Remove from surface by skimming or suitable absorbents.   
      Notify local authorities according to regulations. 
6.4 Reference to other sections 
      Personal precautions: see section 8. Waste treatment methods: see section 13. 

7. Handling and storage
7.1 Precautions for safe handling
      Protective measures: wear personal protective equipment. Avoid contact with skin and eyes. Avoid 
      prolonged breathing of oil vapours or mists. If sprayed, it is preferable to use a full-face visor or   
      special chemical goggles. In case vapours and mist is formed respiratory equipment with a  
      suitable filter will be used. Do not spill the product.
      Hygiene measures: Smoking, eating and drinking are prohibited in the area where the product is 
      used. Wash hands before breaks and at the end of the work schedule. Wear oil resistant footwear   
      and protective gloves. Wash contaminated clothing with soap and water.
      Fire prevention measures: Keep away from heat and other sources of ignition.
7.2 Conditions for safe storage, including any incompatibilities 
      Storage facilities must comply with regulations for storing of flammable liquids. Store in dry, well- 
      ventilated place in original, closed containers. Keep away from radiant heat, open flame and strong 
      oxidizing agents. Storage temperature: Stable if kept between +5°C - +40°C.
7.3 Specific end use(s)
      Recommendations: engine oil.

8. Exposure controls / personal protection
      Engineering control measures: Not required.	
8.1 Control parameters:	
[bookmark: _Hlk63758911]      Pursuant regulations in force, mineral oil mist concentration in air should not exceed 10 mg/m³. 
8.2 Exposure controls	
      Technical measures: see protection measures – Paragraph 7 
      Personal protective equipment: 
      Skin and body protection: Prolonged and repeated contact with skin should be avoided. Otherwise 
      protective measures should be taken. In case of spay hazard use oil-resistant clothing. Soaked 
      clothing and shoes must be changed immediately. Wash skin immediately after work. Do not place 
      dirty or wet rags in pockets. 
      Respiratory protection: In case of exposure above the permissible concentration limit, wear suitable 
      respiratory equipment.
      Hand protection: Oil resistant gloves (EN 374, Breakthrough time 480 min) (e.g. nitrile rubber -  
      minimal thickness 0.33 mm). Note: Manufacturer’s directions for use and the conditions of
      application should be observed.
      Eye protection: In case of a spray hazard use tightly fitting safety goggles.
8.3 Environmental exposure controls:
      Do not discharge into drains/surface waters/groundwater. If the product contaminates rivers, lakes 
      or sewers, the competent authorities shall be notified in accordance with the legal provisions in force. 
      If the product has infested the environment, inform immediately the competent authorities

9.  Physical and chemical properties
9.1 Information on basic physical and chemical properties	
            Appearance:		                      liquid
	Colour:	                                  brown, clear
	Odour:	                                              characteristic of petroleum products
	Odour threshold:                               no
	pH                                                     not applicable
            Melting point:                                   not applicable
            Pour point:                                        - 43 ℃
            Boiling point:	                                   not applicable
            Flash point:	                                   210 ℃ 
	Evaporation rate:                               not applicable
	Flammability:                                    not in normal conditions
	Upper flammability limit:                 not applicable
            Lower flammability limit:                not applicable
            Vapour pressure at 20℃:                  negligible 
            Vapour density:                                 not applicable
            Relative density at 15℃:                   0.870 g/cm³
            Solubility in water at 20℃:               practically insoluble in water
            n-Octanol/water partition 
            coefficient:	                                   not available
            Autoignition temperature:	            not applicable
            Decomposition temperature:             not applicable
            Kinematic viscosity at 40°C:             30 – 90 mm²/s 
            Kinematic viscosity at 100℃:           9.3 – 12.5 mm²/s
	Explosive properties:	                        no
	Oxidizing properties:	                        no
9.2 Other information: no data available
            Soluble in other solvents:                  gasoline, kerosene, toluene                             

10. Stability and reactivity
10.1 Reactivity: Dangerous reactivity not known.
10.2 Chemical stability: No decomposition if stored and handled properly.
10.3 Possibility of hazardous reactions: Not known.
10.4 Conditions to avoid: Direct heat or ignition sources.
10.5 Incompatible materials: Strong oxidizing agents.
10.6 Hazardous decomposition products: No dangerous decomposition products are formed under 
normal conditions. Hazardous combustion products: See Section 5. 

11. Toxicological information
11.1 Information on toxicological effects
      Acute toxicity:				
      Oral:         LD50 (rats)	  > 5000 mg/kg
      Dermal:	LD50 (rabbits) > 2000 mg/kg 
      Acute toxicity: irritation
      Skin:            not irritant 
      Eye:             not irritant 
      Respiratory or skin sensitisation: not sensitising 
      Germ cell mutagenicity: not mutagen 
      Carcinogenicity: not known 
      Reproductive toxicity: not known 
      STOT-single exposure: not known
      STOT-repeated exposure: not known 
      Aspiration hazard: not known.

12. Ecological information
12.1 Toxicity	
        Oral:      LD50 (rats)      > 5000mg/kg (based on components)
        Dermal: LD50 (rabbits) > 2000 mg/kg (based on components)
12.2 Persistence and degradability:	No data available.
        Biodegradability:	            No data available.
12.3 Bio accumulative potential:	No data available.
12.4 Mobility	
        Mobility in soil:   	            Absorbs in soil.
        Mobility in water:	            Floats on water.
12.5 Results of PBT  and  vPvB	Not required.
        assessment	
12.6 Other adverse effects	
        Heavy metal content:	            None.
        PCT, PCB and other 
        chlorinated hydrocarbons:         None.
        Environmental effects:	            Avoid release into underground waters, surface water, sewers.
                                                           Can be mechanically removed from water.	

13. Disposal considerations					
13.1 Waste treatment methods					
13.1.1 Product disposal / Packaging
           Wastes of the product or used oil should be treated as hazardous waste. EWC code: 13 02 05* 
           Disposal must be in compliance with national and local regulations. 
           Packaging disposal: Containers with product residue should also be treated as hazardous 
           waste according to national and local disposal regulations. EWC code: 15 01 10* 
13.1.2 Packaging containing residues of, or contaminated by dangerous substances. 
           Disposal must be in compliance with national and local regulations. 
13.1.3 Wastewater: Quality of wastewater emitted to natural water must comply with national and 
           local regulations. Sewer disposal is forbidden.
13.1.4 Other recommendations: 
           Care should be taken in any case to ensure compliance with EC, national and local regulations. 
           It is the responsibility of the user to know all relevant national and local regulations. 

14.  Transport information 
       Land transport: 
       Road/ Railway	                         ADR/RID:	            Not classified.
       Waterways:		
       Inland waterways/ Sea transport  ADN/IMDG:		Not classified.
       Air transport:	                         ICAO / IATA:	Not classified.

15. Regulatory information 
15.1 Safety, health and environmental regulations/legislation specific for the mixture. 
        Relevant Romanian regulation and EU directives 
        - Directive 94/33 / EC on the protection of young people at work.
        - Directive 92/85 / EEC on the safety and health at work of pregnant women.
        - Regulation (EC) No 1272/2008 [CLP]
        - Law no. 360/2003 on the regime of dangerous chemical substances and mixtures.
        - Law no. 263/2005 for the amendment, completion of Law no. 360/2003 regarding the regime of
          hazardous chemicals and preparations.
        -GD 856/2002 On the record of waste management and the approval of the list containing waste, 
          including hazardous waste.
        - GD 188/2002 Approval of some norms regarding the discharge conditions of wastewaters in the
          aquatic environment 
        - GD 352/2005 Modification and completion of GD 188/2002 for the approval of some norms 
          regarding conditions for the discharge of wastewater into the aquatic environment.
        - GD 235/2007 Waste oils management.
15.2 Chemical safety assessment. 
        Not available 

16. Other information 
      The full text of each relevant R-, H- phrase and Hazard classes and cat. in Sections 2 and 3: 
P 273: Avoid release to the environment.
P 501: Dispose of contents/container in accordance with national regulation.	
H 315: Causes skin irritation.	
H 317: May cause an allergic skin reaction.
H 318: Causes serious eye damage.
H 361: Suspected of damaging fertility or the unborn child.
H 411: Toxic to aquatic life with long lasting effects.

The information given in this data sheet is based on our best knowledge at the time of publication. 
This information is given for information purposes and is intended to assist its safe handling, 
storage, transport, distribution, proper safe use and disposal and therefore cannot be considered as a 
quality or guarantee certificate. The information refers only to the specified product and will not be valid 
when the product is  combined with any other products or in any manufacturing process without express
specification.
The manufacturer or supplier shall not take responsibility for any damages from the use other than
recommended or other misuse of the product. It is the responsibility of the user to keep regulatory 
precautions and observe recommendations for safe use of the product. 
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